2025-11-21 15:10:39.661724

---------------------------------------------------------------------------------------------------------------------------
> re 

Hardware inventory:

Item             Version  Part number  Serial number     Description

Chassis                                AN10567276        QFX5120-32C

Pseudo CB 0     

Routing Engine 0          BUILTIN      BUILTIN           RE-QFX5120-32C

FPC 0            REV 05   650-092914   AN10567276        QFX5120-32C

  CPU                     BUILTIN      BUILTIN           FPC CPU

  PIC 0                   BUILTIN      BUILTIN           32X40G/32X100G-QSFP

    Xcvr 0       C        NON-JNPR     231211W0022       QSFP-100GBASE-SR4

Power Supply 0   REV 01   640-084631   1GG1D060584       QFX520048Y-650W-AC-AFO

Power Supply 1   REV 01   640-084631   1GG1D060587       QFX520048Y-650W-AC-AFO

Fan Tray 0                                               QFX5120-32C Fan Tray 0, Front to Back Airflow - AFO

Fan Tray 1                                               QFX5120-32C Fan Tray 1, Front to Back Airflow - AFO

Fan Tray 2                                               QFX5120-32C Fan Tray 2, Front to Back Airflow - AFO

Fan Tray 3                                               QFX5120-32C Fan Tray 3, Front to Back Airflow - AFO

Fan Tray 4                                               QFX5120-32C Fan Tray 4, Front to Back Airflow - AFO

Fan Tray 5                                               QFX5120-32C Fan Tray 5, Front to Back Airflow - AFO



{master:0}

root@LAB_QFX5120-32C> /0 

et-0/0/0                up    up

et-0/0/0.0              up    up   inet     10.10.10.1/24   



{master:0}

root@LAB_QFX5120-32C> re 

Physical interface: et-0/0/0, Enabled, Physical link is Up

  Interface index: 650, SNMP ifIndex: 506

  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 100Gbps, BPDU Error: None, Loop Detect PDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Media type: Fiber

  Device flags   : Present Running

  Interface flags: SNMP-Traps Internal: 0x4000

  Link flags     : None

  CoS queues     : 10 supported, 10 maximum usable queues

  Current address: 48:5a:0d:b5:1c:57, Hardware address: 48:5a:0d:b5:1c:57

  Last flapped   : 2023-07-26 13:06:20 UTC (00:00:20 ago)

  Input rate     : 1000 bps (1 pps)

  Output rate    : 1000 bps (1 pps)

  Active alarms  : None

  Active defects : None

 Pre-emphasis(reg 236/237)

                       Register-value                 0

 Ctle(reg 234/235)

                    Register-value                 0

 Differential-amplitude(reg 238/239)

                        Register-value                 0

  PCS statistics                      Seconds

    Bit errors                             0

    Errored blocks                         0

  Ethernet FEC Mode  :                  FEC91

  Ethernet FEC statistics              Errors

    FEC Corrected Errors                    0

    FEC Uncorrected Errors                  0

    FEC Corrected Errors Rate               0

    FEC Uncorrected Errors Rate             0

  PRBS Mode : Disabled

  Interface transmit statistics: Disabled



  Logical interface et-0/0/0.0 (Index 554) (SNMP ifIndex 519)

    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2

    Input packets : 32

    Output packets: 23

    Protocol inet, MTU: 1500

    Max nh cache: 75000, New hold nh limit: 75000, Curr nh cnt: 1, Curr new hold cnt: 0, NH drop cnt: 0

      Flags: Sendbcast-pkt-to-re, Is-Primary

      Addresses, Flags: Is-Default Is-Preferred Is-Primary

        Destination: 10.10.10/24, Local: 10.10.10.1, Broadcast: 10.10.10.255



{master:0}

root@LAB_QFX5120-32C> re 

Physical interface: et-0/0/0, Enabled, Physical link is Up

  Interface index: 650, SNMP ifIndex: 506, Generation: 154

  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 100Gbps, BPDU Error: None, Loop Detect PDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Media type: Fiber

  Device flags   : Present Running

  Interface flags: SNMP-Traps Internal: 0x4000

  Link flags     : None

  CoS queues     : 10 supported, 10 maximum usable queues

  Hold-times     : Up 0 ms, Down 0 ms

  Current address: 48:5a:0d:b5:1c:57, Hardware address: 48:5a:0d:b5:1c:57

  Last flapped   : 2023-07-26 13:06:20 UTC (00:00:24 ago)

  Statistics last cleared: Never

  Traffic statistics:

   Input  bytes  :                 3394                 1000 bps

   Output bytes  :                 2334                 1000 bps

   Input  packets:                   36                    1 pps

   Output packets:                   24                    1 pps

   IPv6 transit statistics:

   Input  bytes  :                    0

   Output bytes  :                    0

   Input  packets:                    0

   Output packets:                    0

  Input errors:

    Errors: 0, Drops: 0, Framing errors: 0, Runts: 0, Policed discards: 0, L3 incompletes: 0, L2 channel errors: 0, L2 mismatch timeouts: 0, FIFO errors: 0, Resource errors: 0

  Output errors:

    Carrier transitions: 1, Errors: 0, Drops: 0, Collisions: 0, Aged packets: 0, FIFO errors: 0, HS link CRC errors: 0, MTU errors: 0, Resource errors: 0

  Egress queues: 10 supported, 5 in use

  Queue counters:       Queued packets  Transmitted packets      Dropped packets

    0                               25                   25                    0

    3                                0                    0                    0

    4                                0                    0                    0

    7                                0                    0                    0

    8                                0                    0                    0

  Queue number:         Mapped forwarding classes

    0                   best-effort

    3                   fcoe

    4                   no-loss

    7                   network-control

    8                   mcast

  Active alarms  : None

  Active defects : None

 Pre-emphasis(reg 236/237)

                       Register-value                 0

 Ctle(reg 234/235)

                    Register-value                 0

 Differential-amplitude(reg 238/239)

                        Register-value                 0

  PCS statistics                      Seconds

    Bit errors                             0

    Errored blocks                         0

  Ethernet FEC Mode  :                  FEC91

  Ethernet FEC statistics              Errors

    FEC Corrected Errors                    0

    FEC Uncorrected Errors                  0

    FEC Corrected Errors Rate               0

    FEC Uncorrected Errors Rate             0

  MAC statistics:                      Receive         Transmit

    Total octets                          3394             2334

    Total packets                           36               24

    Unicast packets                         24               22

    Broadcast packets                        4                2

    Multicast packets                        8                0

    CRC/Align errors                         0                0

    FIFO errors                              0                0

    MAC control frames                       0                0

    MAC pause frames                         0                0

    Oversized frames                         0

    Jabber frames                            0

    Fragment frames                          0

    VLAN tagged frames                       0

    Code violations                          0

  MAC Priority Flow Control Statistics:

    Priority :  0                             0                0

    Priority :  1                             0                0

    Priority :  2                             0                0

    Priority :  3                             0                0

    Priority :  4                             0                0

    Priority :  5                             0                0

    Priority :  6                             0                0

    Priority :  7                             0                0

  PRBS Mode : Disabled

  Packet Forwarding Engine configuration:

    Destination slot: 0 (0x00)

  CoS information:

    Direction : Output

    CoS transmit queue               Bandwidth               Buffer Priority   Limit

                              %            bps     %           usec

    0 best-effort             5     5000000000     5              0      low    none

    3 fcoe                   35    35000000000    35              0      low    none

    4 no-loss                35    35000000000    35              0      low    none

    7 network-control         5     5000000000     5              0      low    none

    8 mcast                  20    20000000000    20              0      low    none

  Interface transmit statistics: Disabled

  MACSec statistics:

    Output

        Secure Channel Transmitted

        Protected Packets               : 0

        Encrypted Packets               : 0

        Protected Bytes                 : 0

        Encrypted Bytes                 : 0

     Input

        Secure Channel Received

        Accepted Packets                : 0

        Validated Bytes                 : 0

        Decrypted Bytes                 : 0



  Logical interface et-0/0/0.0 (Index 554) (SNMP ifIndex 519) (HW Token 4095) (Generation 152)

    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2

    Traffic statistics:

     Input  bytes  :                 3282

     Output bytes  :                 2478

     Input  packets:                   36

     Output packets:                   27

    Local statistics:

     Input  bytes  :                 2894

     Output bytes  :                 2478

     Input  packets:                   36

     Output packets:                   27

    Transit statistics:

     Input  bytes  :                  388                  808 bps

     Output bytes  :                    0                    0 bps

     Input  packets:                    0                    0 pps

     Output packets:                    0                    0 pps

    Protocol inet, MTU: 1500

    Max nh cache: 75000, New hold nh limit: 75000, Curr nh cnt: 1, Curr new hold cnt: 0, NH drop cnt: 0

    Generation: 172, Route table: 0

      Flags: Sendbcast-pkt-to-re, Is-Primary

      Addresses, Flags: Is-Default Is-Preferred Is-Primary

        Destination: 10.10.10/24, Local: 10.10.10.1, Broadcast: 10.10.10.255, Generation: 162



{master:0}

root@LAB_QFX5120-32C> ore 

  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 100Gbps, BPDU Error: None, Loop Detect PDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Media type: Fiber

  Input errors:

    Errors: 0, Drops: 0, Framing errors: 0, Runts: 0, Policed discards: 0, L3 incompletes: 0, L2 channel errors: 0, L2 mismatch timeouts: 0, FIFO errors: 0, Resource errors: 0

  Output errors:

    Carrier transitions: 1, Errors: 0, Drops: 0, Collisions: 0, Aged packets: 0, FIFO errors: 0, HS link CRC errors: 0, MTU errors: 0, Resource errors: 0

    Bit errors                             0

    Errored blocks                         0

  Ethernet FEC statistics              Errors

    FEC Corrected Errors                    0

    FEC Uncorrected Errors                  0

    FEC Corrected Errors Rate               0

    FEC Uncorrected Errors Rate             0

    CRC/Align errors                         0                0

    FIFO errors                              0                0

      Addresses, Flags: Is-Default Is-Preferred Is-Primary



{master:0}

root@LAB_QFX5120-32C> te 

  Input rate     : 496 bps (0 pps)

  Output rate    : 496 bps (0 pps)

    FEC Corrected Errors Rate               0

    FEC Uncorrected Errors Rate             0

  Input rate     : 0 bps (0 pps)

  Output rate    : 0 bps (0 pps)



{master:0}

root@LAB_QFX5120-32C> re 

Physical interface: et-0/0/0

    Module temperature                        :  27 degrees C / 81 degrees F

    Module voltage                            :  3.2470 V

    Module temperature high alarm             :  Off

    Module temperature low alarm              :  Off

    Module temperature high warning           :  Off

    Module temperature low warning            :  Off

    Module voltage high alarm                 :  Off

    Module voltage low alarm                  :  Off

    Module voltage high warning               :  Off

    Module voltage low warning                :  Off

    Module temperature high alarm threshold   :  85 degrees C / 185 degrees F

    Module temperature low alarm threshold    :  -10 degrees C / 14 degrees F

    Module temperature high warning threshold :  70 degrees C / 158 degrees F

    Module temperature low warning threshold  :  0 degrees C / 32 degrees F

    Module voltage high alarm threshold       :  3.5990 V

    Module voltage low alarm threshold        :  2.9000 V

    Module voltage high warning threshold     :  3.4990 V

    Module voltage low warning threshold      :  3.0990 V

    Laser bias current high alarm threshold   :  14.999 mA

    Laser bias current low alarm threshold    :  0.999 mA

    Laser bias current high warning threshold :  11.999 mA

    Laser bias current low warning threshold  :  1.999 mA

    Laser output power high alarm threshold   :  2.5119 mW / 4.00 dBm

    Laser output power low alarm threshold    :  0.0871 mW / -10.60 dBm

    Laser output power high warning threshold :  1.7378 mW / 2.40 dBm

    Laser output power low warning threshold  :  0.1738 mW / -7.60 dBm

    Laser rx power high alarm threshold       :  2.5119 mW / 4.00 dBm

    Laser rx power low alarm threshold        :  0.0158 mW / -18.01 dBm

    Laser rx power high warning threshold     :  1.7378 mW / 2.40 dBm

    Laser rx power low warning threshold      :  0.0316 mW / -15.00 dBm

  Lane 0

    Laser bias current                        :  6.288 mA

    Laser output power                        :  1.061 mW / 0.26 dBm

    Laser receiver power                      :  1.200 mW / 0.79 dBm

    Laser bias current high alarm             :  Off

    Laser bias current low alarm              :  Off

    Laser bias current high warning           :  Off

    Laser bias current low warning            :  Off

    Laser receiver power high alarm           :  Off

    Laser receiver power low alarm            :  Off

    Laser receiver power high warning         :  Off

    Laser receiver power low warning          :  Off

    Tx loss of signal functionality alarm     :  Off

    Rx loss of signal alarm                   :  Off

    Tx laser disabled alarm                   :  Off

  Lane 1

    Laser bias current                        :  6.280 mA

    Laser output power                        :  1.085 mW / 0.36 dBm

    Laser receiver power                      :  1.247 mW / 0.96 dBm

    Laser bias current high alarm             :  Off

    Laser bias current low alarm              :  Off

    Laser bias current high warning           :  Off

    Laser bias current low warning            :  Off

    Laser receiver power high alarm           :  Off

    Laser receiver power low alarm            :  Off

    Laser receiver power high warning         :  Off

    Laser receiver power low warning          :  Off

    Tx loss of signal functionality alarm     :  Off

    Rx loss of signal alarm                   :  Off

    Tx laser disabled alarm                   :  Off

  Lane 2

    Laser bias current                        :  6.320 mA

    Laser output power                        :  1.066 mW / 0.28 dBm

    Laser receiver power                      :  1.059 mW / 0.25 dBm

    Laser bias current high alarm             :  Off

    Laser bias current low alarm              :  Off

    Laser bias current high warning           :  Off

    Laser bias current low warning            :  Off

    Laser receiver power high alarm           :  Off

    Laser receiver power low alarm            :  Off

    Laser receiver power high warning         :  Off

    Laser receiver power low warning          :  Off

    Tx loss of signal functionality alarm     :  Off

    Rx loss of signal alarm                   :  Off

    Tx laser disabled alarm                   :  Off

  Lane 3

    Laser bias current                        :  6.300 mA

    Laser output power                        :  1.205 mW / 0.81 dBm

    Laser receiver power                      :  1.205 mW / 0.81 dBm

    Laser bias current high alarm             :  Off

    Laser bias current low alarm              :  Off

    Laser bias current high warning           :  Off

    Laser bias current low warning            :  Off

    Laser receiver power high alarm           :  Off

    Laser receiver power low alarm            :  Off

    Laser receiver power high warning         :  Off

    Laser receiver power low warning          :  Off

    Tx loss of signal functionality alarm     :  Off

    Rx loss of signal alarm                   :  Off

    Tx laser disabled alarm                   :  Off



{master:0}

root@LAB_QFX5120-32C> ore 

Physical interface: et-0/0/0

    Module temperature                        :  28 degrees C / 82 degrees F

    Module voltage                            :  3.2730 V

    Module temperature high alarm threshold   :  85 degrees C / 185 degrees F

    Module temperature low alarm threshold    :  -10 degrees C / 14 degrees F

    Module temperature high warning threshold :  70 degrees C / 158 degrees F

    Module temperature low warning threshold  :  0 degrees C / 32 degrees F

    Module voltage high alarm threshold       :  3.5990 V

    Module voltage low alarm threshold        :  2.9000 V

    Module voltage high warning threshold     :  3.4990 V

    Module voltage low warning threshold      :  3.0990 V

    Laser bias current high alarm threshold   :  14.999 mA

    Laser bias current low alarm threshold    :  0.999 mA

    Laser bias current high warning threshold :  11.999 mA

    Laser bias current low warning threshold  :  1.999 mA

    Laser output power high alarm threshold   :  2.5119 mW / 4.00 dBm

    Laser output power low alarm threshold    :  0.0871 mW / -10.60 dBm

    Laser output power high warning threshold :  1.7378 mW / 2.40 dBm

    Laser output power low warning threshold  :  0.1738 mW / -7.60 dBm

    Laser rx power high alarm threshold       :  2.5119 mW / 4.00 dBm

    Laser rx power low alarm threshold        :  0.0158 mW / -18.01 dBm

    Laser rx power high warning threshold     :  1.7378 mW / 2.40 dBm

    Laser rx power low warning threshold      :  0.0316 mW / -15.00 dBm

  Lane 0

    Laser bias current                        :  6.306 mA

    Laser output power                        :  1.064 mW / 0.27 dBm

    Laser receiver power                      :  1.211 mW / 0.83 dBm

  Lane 1

    Laser bias current                        :  6.300 mA

    Laser output power                        :  1.089 mW / 0.37 dBm

    Laser receiver power                      :  1.255 mW / 0.99 dBm

  Lane 2

    Laser bias current                        :  6.291 mA

    Laser output power                        :  1.061 mW / 0.26 dBm

    Laser receiver power                      :  1.055 mW / 0.23 dBm

  Lane 3

    Laser bias current                        :  6.285 mA

    Laser output power                        :  1.203 mW / 0.80 dBm

    Laser receiver power                      :  1.207 mW / 0.82 dBm



{master:0}

root@LAB_QFX5120-32C> 0 

PING 10.10.10.2 (10.10.10.2): 56 data bytes

!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!

--- 10.10.10.2 ping statistics ---

200 packets transmitted, 200 packets received, 0% packet loss

round-trip min/avg/max/stddev = 0.737/7.610/10.613/1.756 ms



{master:0}

root@LAB_QFX5120-32C