{master:0}
root@LAB_QFX5120-32C> ping 10.10.10.20 in
                                         ^
'in' is ambiguous.
Possible completions:
  inet                 Force ping to IPv4 destination
  inet6                Force ping to IPv6 destination
  interface            Source interface (multicast, all-ones, unrouted packets)
  interval             Delay between ping requests (seconds)
root@LAB_QFX5120-32C> ping 10.10.10.20 interface irb.11 
PING 10.10.10.20 (10.10.10.20): 56 data bytes
64 bytes from 10.10.10.20: icmp_seq=0 ttl=64 time=3.121 ms
64 bytes from 10.10.10.20: icmp_seq=1 ttl=64 time=4.036 ms
^C
--- 10.10.10.20 ping statistics ---
2 packets transmitted, 2 packets received, 0% packet loss
round-trip min/avg/max/stddev = 3.121/3.579/4.036/0.457 ms

{master:0}
root@LAB_QFX5120-32C> ping 10.10.10.20 interface irb.11 rapid count 100 
PING 10.10.10.20 (10.10.10.20): 56 data bytes
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
--- 10.10.10.20 ping statistics ---
100 packets transmitted, 100 packets received, 0% packet loss
round-trip min/avg/max/stddev = 0.295/5.966/11.619/3.514 ms

{master:0}
root@LAB_QFX5120-32C> show lacp interfaces ae10 
Aggregated interface: ae10
    LACP state:       Role   Exp   Def  Dist  Col  Syn  Aggr  Timeout  Activity
      et-0/0/0       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/0     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
      et-0/0/2       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/2     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
    LACP protocol:        Receive State  Transmit State          Mux State 
      et-0/0/0                  Current   Slow periodic Collecting distributing
      et-0/0/2                  Current   Slow periodic Collecting distributing

{master:0}
root@LAB_QFX5120-32C> show interfaces ae10 
Physical interface: ae10, Enabled, Physical link is Up
  Interface index: 652, SNMP ifIndex: 522
  Link-level type: Ethernet, MTU: 1514, Speed: 200Gbps, BPDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Current address: 48:5a:0d:b5:1d:14, Hardware address: 48:5a:0d:b5:1d:14
  Last flapped   : 2023-07-26 15:00:32 UTC (00:16:40 ago)
  Input rate     : 3504 bps (3 pps)
  Output rate    : 1000 bps (1 pps)

  Logical interface ae10.0 (Index 554) (SNMP ifIndex 523)
    Flags: Up SNMP-Traps 0x24024000 Encapsulation: Ethernet-Bridge
    Statistics        Packets        pps         Bytes          bps
    Bundle:
        Input :             0          0             0            0
        Output:           576          0         54216            0
    Adaptive Statistics:
        Adaptive Adjusts:          0
        Adaptive Scans  :          0
        Adaptive Updates:          0
    Protocol eth-switch, MTU: 1514
      Flags: Is-Primary

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> show lacp interfaces ae10                            
Aggregated interface: ae10
    LACP state:       Role   Exp   Def  Dist  Col  Syn  Aggr  Timeout  Activity
      et-0/0/0       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/0     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
      et-0/0/2       Actor    No    No    No   No   No   Yes     Fast    Active
      et-0/0/2     Partner    No    No    No   No  Yes   Yes     Slow    Active
    LACP protocol:        Receive State  Transmit State          Mux State 
      et-0/0/0                  Current   Slow periodic Collecting distributing
      et-0/0/2                  Current   Slow periodic            Waiting

{master:0}
root@LAB_QFX5120-32C> show lacp interfaces ae10    
Aggregated interface: ae10
    LACP state:       Role   Exp   Def  Dist  Col  Syn  Aggr  Timeout  Activity
      et-0/0/0       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/0     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
      et-0/0/2       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/2     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
    LACP protocol:        Receive State  Transmit State          Mux State 
      et-0/0/0                  Current   Slow periodic Collecting distributing
      et-0/0/2                  Current   Slow periodic Collecting distributing

{master:0}
root@LAB_QFX5120-32C> ping 10.10.10.20 interface irb.11 rapid count 100    
PING 10.10.10.20 (10.10.10.20): 56 data bytes
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
--- 10.10.10.20 ping statistics ---
100 packets transmitted, 100 packets received, 0% packet loss
round-trip min/avg/max/stddev = 0.364/6.268/48.075/5.196 ms

{master:0}
root@LAB_QFX5120-32C> show interfaces ae10 
Physical interface: ae10, Enabled, Physical link is Up
  Interface index: 652, SNMP ifIndex: 522
  Link-level type: Ethernet, MTU: 1514, Speed: 200Gbps, BPDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Current address: 48:5a:0d:b5:1d:14, Hardware address: 48:5a:0d:b5:1d:14
  Last flapped   : 2023-07-26 15:20:47 UTC (00:00:26 ago)
  Input rate     : 3512 bps (3 pps)
  Output rate    : 1000 bps (1 pps)

  Logical interface ae10.0 (Index 554) (SNMP ifIndex 523)
    Flags: Up SNMP-Traps 0x24024000 Encapsulation: Ethernet-Bridge
    Statistics        Packets        pps         Bytes          bps
    Bundle:
        Input :             0          0             0            0
        Output:           784          0         75096            0
    Adaptive Statistics:
        Adaptive Adjusts:          0
        Adaptive Scans  :          0
        Adaptive Updates:          0
    Protocol eth-switch, MTU: 1514
      Flags: Is-Primary

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> show lacp interfaces ae10                            
Aggregated interface: ae10
    LACP state:       Role   Exp   Def  Dist  Col  Syn  Aggr  Timeout  Activity
      et-0/0/0       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/0     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
      et-0/0/2       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/2     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
    LACP protocol:        Receive State  Transmit State          Mux State 
      et-0/0/0                  Current   Slow periodic Collecting distributing
      et-0/0/2                  Current   Slow periodic Collecting distributing

{master:0}
root@LAB_QFX5120-32C> ping 10.10.10.20 interface irb.11 rapid count 100    
PING 10.10.10.20 (10.10.10.20): 56 data bytes
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
--- 10.10.10.20 ping statistics ---
100 packets transmitted, 100 packets received, 0% packet loss
round-trip min/avg/max/stddev = 0.238/5.237/27.625/4.280 ms

{master:0}
root@LAB_QFX5120-32C> show lacp interfaces ae10                            
Aggregated interface: ae10
    LACP state:       Role   Exp   Def  Dist  Col  Syn  Aggr  Timeout  Activity
      et-0/0/0       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/0     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
      et-0/0/2       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/2     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
    LACP protocol:        Receive State  Transmit State          Mux State 
      et-0/0/0                  Current   Slow periodic Collecting distributing
      et-0/0/2                  Current   Slow periodic Collecting distributing

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> show lacp interfaces ae10                            
Aggregated interface: ae10
    LACP state:       Role   Exp   Def  Dist  Col  Syn  Aggr  Timeout  Activity
      et-0/0/0       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/0     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
      et-0/0/2       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/2     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
    LACP protocol:        Receive State  Transmit State          Mux State 
      et-0/0/0                  Current   Slow periodic Collecting distributing
      et-0/0/2                  Current   Slow periodic Collecting distributing

{master:0}
root@LAB_QFX5120-32C> ping 10.10.10.20 interface irb.11 rapid count 100    
PING 10.10.10.20 (10.10.10.20): 56 data bytes
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
--- 10.10.10.20 ping statistics ---
100 packets transmitted, 100 packets received, 0% packet loss
round-trip min/avg/max/stddev = 1.239/7.999/43.465/3.829 ms

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> show interfaces ae10                                 
Physical interface: ae10, Enabled, Physical link is Up
  Interface index: 652, SNMP ifIndex: 522
  Link-level type: Ethernet, MTU: 1514, Speed: 200Gbps, BPDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Current address: 48:5a:0d:b5:1d:14, Hardware address: 48:5a:0d:b5:1d:14
  Last flapped   : 2023-07-26 15:27:19 UTC (00:01:12 ago)
  Input rate     : 3488 bps (3 pps)
  Output rate    : 992 bps (1 pps)

  Logical interface ae10.0 (Index 554) (SNMP ifIndex 523)
    Flags: Up SNMP-Traps 0x24024000 Encapsulation: Ethernet-Bridge
    Statistics        Packets        pps         Bytes          bps
    Bundle:
        Input :             0          0             0            0
        Output:          1285          0        125134            0
    Adaptive Statistics:
        Adaptive Adjusts:          0
        Adaptive Scans  :          0
        Adaptive Updates:          0
    Protocol eth-switch, MTU: 1514
      Flags: Is-Primary

{master:0}
root@LAB_QFX5120-32C> show interfaces ae10 extensive 
Physical interface: ae10, Enabled, Physical link is Up
  Interface index: 652, SNMP ifIndex: 522, Generation: 162
  Link-level type: Ethernet, MTU: 1514, Speed: 200Gbps, BPDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Current address: 48:5a:0d:b5:1d:14, Hardware address: 48:5a:0d:b5:1d:14
  Last flapped   : 2023-07-26 15:27:19 UTC (00:01:16 ago)
  Statistics last cleared: Never
  Traffic statistics:
   Input  bytes  :                34870                 3520 bps
   Output bytes  :                19822                 1000 bps
   Input  packets:                  306                    3 pps
   Output packets:                  192                    1 pps
   IPv6 transit statistics:
   Input  bytes  :                    0
   Output bytes  :                    0
   Input  packets:                    0
   Output packets:                    0
  Input errors:
    Errors: 0, Drops: 0, Framing errors: 0, Runts: 0, Giants: 0, Policed discards: 0, Resource errors: 0
  Output errors:
    Carrier transitions: 2, Errors: 0, Drops: 0, MTU errors: 0, Resource errors: 0
  Egress queues: 10 supported, 5 in use
  Queue counters:       Queued packets  Transmitted packets      Dropped packets
    0                              176                  176                    0
    3                                0                    0                    0
    4                                0                    0                    0
    7                               15                   15                    0
    8                                0                    0                    0
  Queue number:         Mapped forwarding classes
    0                   best-effort
    3                   fcoe
    4                   no-loss
    7                   network-control
    8                   mcast

  Logical interface ae10.0 (Index 554) (SNMP ifIndex 523) (HW Token 1) (Generation 166)
    Flags: Up SNMP-Traps 0x24024000 Encapsulation: Ethernet-Bridge
    Statistics        Packets        pps         Bytes          bps
    Bundle:
        Input :             0          0             0            0
        Output:          1289          0        125542            0
    Adaptive Statistics:
        Adaptive Adjusts:          0
        Adaptive Scans  :          0
        Adaptive Updates:          0
    Link:                               
      et-0/0/0.0
        Input :             0          0             0            0
        Output:           179          0         18034            0
      et-0/0/2.0
        Input :             0          0             0            0
        Output:             0          0             0            0


    Aggregate member links: 2

    LACP info:        Role     System             System       Port     Port    Port 
                             priority         identifier   priority   number     key 
      et-0/0/0.0     Actor        127  48:5a:0d:b5:1c:54        127        1      11
      et-0/0/0.0   Partner      65535  88:e9:a4:8e:63:d2        255        1      29
      et-0/0/2.0     Actor        127  48:5a:0d:b5:1c:54        127        2      11
      et-0/0/2.0   Partner      65535  88:e9:a4:8e:63:d2        255        2      29
    LACP Statistics:       LACP Rx     LACP Tx   Unknown Rx   Illegal Rx 
      et-0/0/0.0                48           7            0            0
      et-0/0/2.0                21           6            0            0
    Marker Statistics:   Marker Rx     Resp Tx   Unknown Rx   Illegal Rx
      et-0/0/0.0                 0           0            0            0
      et-0/0/2.0                 0           0            0            0
    Protocol eth-switch, MTU: 1514, Generation: 185, Route table: 7, Mesh Group: __all_ces__, Next-hop: 1718, vpls-status: up
      Flags: Is-Primary                 

{master:0}
root@LAB_QFX5120-32C> show interfaces ae10 extensive | match err 
  Link-level type: Ethernet, MTU: 1514, Speed: 200Gbps, BPDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Input errors:
    Errors: 0, Drops: 0, Framing errors: 0, Runts: 0, Giants: 0, Policed discards: 0, Resource errors: 0
  Output errors:
    Carrier transitions: 2, Errors: 0, Drops: 0, MTU errors: 0, Resource errors: 0

{master:0}
root@LAB_QFX5120-32C> show interfaces ae10 extensive | match err    
  Link-level type: Ethernet, MTU: 1514, Speed: 200Gbps, BPDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Input errors:
    Errors: 0, Drops: 0, Framing errors: 0, Runts: 0, Giants: 0, Policed discards: 0, Resource errors: 0
  Output errors:
    Carrier transitions: 2, Errors: 0, Drops: 0, MTU errors: 0, Resource errors: 0

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> show lacp interfaces ae10 
Aggregated interface: ae10
    LACP state:       Role   Exp   Def  Dist  Col  Syn  Aggr  Timeout  Activity
      et-0/0/0       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/0     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
      et-0/0/2       Actor    No    No   Yes  Yes  Yes   Yes     Fast    Active
      et-0/0/2     Partner    No    No   Yes  Yes  Yes   Yes     Slow    Active
    LACP protocol:        Receive State  Transmit State          Mux State 
      et-0/0/0                  Current   Slow periodic Collecting distributing
      et-0/0/2                  Current   Slow periodic Collecting distributing

{master:0}
root@LAB_QFX5120-32C> ping 10.10.10.20 interface irb.11 rapid count 100    
PING 10.10.10.20 (10.10.10.20): 56 data bytes
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
--- 10.10.10.20 ping statistics ---
100 packets transmitted, 100 packets received, 0% packet loss
round-trip min/avg/max/stddev = 0.256/5.836/10.330/3.401 ms

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> 

{master:0}
root@LAB_QFX5120-32C> show interfaces ae10 extensive 
Physical interface: ae10, Enabled, Physical link is Up
  Interface index: 652, SNMP ifIndex: 522, Generation: 162
  Link-level type: Ethernet, MTU: 1514, Speed: 200Gbps, BPDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Device flags   : Present Running
  Interface flags: SNMP-Traps Internal: 0x4000
  Current address: 48:5a:0d:b5:1d:14, Hardware address: 48:5a:0d:b5:1d:14
  Last flapped   : 2023-07-26 15:30:50 UTC (00:00:54 ago)
  Statistics last cleared: Never
  Traffic statistics:
   Input  bytes  :                29562                 3520 bps
   Output bytes  :                17616                 1000 bps
   Input  packets:                  259                    3 pps
   Output packets:                  170                    1 pps
   IPv6 transit statistics:
   Input  bytes  :                    0
   Output bytes  :                    0
   Input  packets:                    0
   Output packets:                    0
  Input errors:
    Errors: 0, Drops: 0, Framing errors: 0, Runts: 0, Giants: 0, Policed discards: 0, Resource errors: 0
  Output errors:
    Carrier transitions: 2, Errors: 0, Drops: 0, MTU errors: 0, Resource errors: 0
  Egress queues: 10 supported, 5 in use
  Queue counters:       Queued packets  Transmitted packets      Dropped packets
    0                              157                  157                    0
    3                                0                    0                    0
    4                                0                    0                    0
    7                               15                   15                    0
    8                                0                    0                    0
  Queue number:         Mapped forwarding classes
    0                   best-effort
    3                   fcoe
    4                   no-loss
    7                   network-control
    8                   mcast

  Logical interface ae10.0 (Index 554) (SNMP ifIndex 523) (HW Token 1) (Generation 166)
    Flags: Up SNMP-Traps 0x24024000 Encapsulation: Ethernet-Bridge
    Statistics        Packets        pps         Bytes          bps
    Bundle:
        Input :             0          0             0            0
        Output:          1488          0        145560            0
    Adaptive Statistics:
        Adaptive Adjusts:          0
        Adaptive Scans  :          0
        Adaptive Updates:          0
    Link:
      et-0/0/0.0
        Input :             0          0             0            0
        Output:           159          0         15994            0
      et-0/0/2.0
        Input :             0          0             0            0
        Output:             0          0             0            0


    Aggregate member links: 2

    LACP info:        Role     System             System       Port     Port    Port 
                             priority         identifier   priority   number     key 
      et-0/0/0.0     Actor        127  48:5a:0d:b5:1c:54        127        1      11
      et-0/0/0.0   Partner      65535  88:e9:a4:8e:63:d2        255        2      29
      et-0/0/2.0     Actor        127  48:5a:0d:b5:1c:54        127        2      11
      et-0/0/2.0   Partner      65535  88:e9:a4:8e:63:d2        255        1      29
    LACP Statistics:       LACP Rx     LACP Tx   Unknown Rx   Illegal Rx 
      et-0/0/0.0                45           8            0            0
      et-0/0/2.0                38           7            0            0
    Marker Statistics:   Marker Rx     Resp Tx   Unknown Rx   Illegal Rx
      et-0/0/0.0                 0           0            0            0
      et-0/0/2.0                 0           0            0            0
    Protocol eth-switch, MTU: 1514, Generation: 185, Route table: 7, Mesh Group: __all_ces__, Next-hop: 1718, vpls-status: up
      Flags: Is-Primary

{master:0}
root@LAB_QFX5120-32C> show interfaces ae10 extensive | match err 
  Link-level type: Ethernet, MTU: 1514, Speed: 200Gbps, BPDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Minimum links needed: 1, Minimum bandwidth needed: 1bps
  Input errors:
    Errors: 0, Drops: 0, Framing errors: 0, Runts: 0, Giants: 0, Policed discards: 0, Resource errors: 0
  Output errors:
    Carrier transitions: 2, Errors: 0, Drops: 0, MTU errors: 0, Resource errors: 0
