2025-11-21 14:49:27.932455

---------------------------------------------------------------------------------------------------------------------------
> ore 

Hardware inventory:

Item             Version  Part number  Serial number     Description

Chassis                                AN10567276        QFX5120-32C

Pseudo CB 0     

Routing Engine 0          BUILTIN      BUILTIN           RE-QFX5120-32C

FPC 0            REV 05   650-092914   AN10567276        QFX5120-32C

  CPU                     BUILTIN      BUILTIN           FPC CPU

  PIC 0                   BUILTIN      BUILTIN           32X40G/32X100G-QSFP

    Xcvr 0                NON-JNPR     240727W0013       QSFP-100GBASE-SR4

Power Supply 0   REV 01   640-084631   1GG1D060584       QFX520048Y-650W-AC-AFO

Power Supply 1   REV 01   640-084631   1GG1D060587       QFX520048Y-650W-AC-AFO

Fan Tray 0                                               QFX5120-32C Fan Tray 0, Front to Back Airflow - AFO

Fan Tray 1                                               QFX5120-32C Fan Tray 1, Front to Back Airflow - AFO

Fan Tray 2                                               QFX5120-32C Fan Tray 2, Front to Back Airflow - AFO

Fan Tray 3                                               QFX5120-32C Fan Tray 3, Front to Back Airflow - AFO

Fan Tray 4                                               QFX5120-32C Fan Tray 4, Front to Back Airflow - AFO

Fan Tray 5                                               QFX5120-32C Fan Tray 5, Front to Back Airflow - AFO



{master:0}

root@LAB_QFX5120-32C> /0 

et-0/0/0                up    up

et-0/0/0.0              up    up   inet     10.10.10.1/24   



{master:0}

root@LAB_QFX5120-32C> ore 

Physical interface: et-0/0/0, Enabled, Physical link is Up

  Interface index: 650, SNMP ifIndex: 506

  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 100Gbps, BPDU Error: None, Loop Detect PDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Media type: Fiber

  Device flags   : Present Running

  Interface flags: SNMP-Traps Internal: 0x4000

  Link flags     : None

  CoS queues     : 10 supported, 10 maximum usable queues

  Current address: 48:5a:0d:b5:1c:57, Hardware address: 48:5a:0d:b5:1c:57

  Last flapped   : 2023-07-26 12:44:34 UTC (00:00:55 ago)

  Input rate     : 992 bps (1 pps)

  Output rate    : 992 bps (1 pps)

  Active alarms  : None

  Active defects : None

 Pre-emphasis(reg 236/237)

                       Register-value                 0

 Ctle(reg 234/235)

                    Register-value                 0

 Differential-amplitude(reg 238/239)

                        Register-value                 0

  PCS statistics                      Seconds

    Bit errors                             0

    Errored blocks                         0

  Ethernet FEC Mode  :                  FEC91

  Ethernet FEC statistics              Errors

    FEC Corrected Errors                    0

    FEC Uncorrected Errors                  0

    FEC Corrected Errors Rate               0

    FEC Uncorrected Errors Rate             0

  PRBS Mode : Disabled

  Interface transmit statistics: Disabled



  Logical interface et-0/0/0.0 (Index 554) (SNMP ifIndex 519)

    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2

    Input packets : 68

    Output packets: 59

    Protocol inet, MTU: 1500

    Max nh cache: 75000, New hold nh limit: 75000, Curr nh cnt: 1, Curr new hold cnt: 0, NH drop cnt: 0

      Flags: Sendbcast-pkt-to-re, Is-Primary

      Addresses, Flags: Is-Default Is-Preferred Is-Primary

        Destination: 10.10.10/24, Local: 10.10.10.1, Broadcast: 10.10.10.255



{master:0}

root@LAB_QFX5120-32C> e 

Physical interface: et-0/0/0, Enabled, Physical link is Up

  Interface index: 650, SNMP ifIndex: 506, Generation: 143

  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 100Gbps, BPDU Error: None, Loop Detect PDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Media type: Fiber

  Device flags   : Present Running

  Interface flags: SNMP-Traps Internal: 0x4000

  Link flags     : None

  CoS queues     : 10 supported, 10 maximum usable queues

  Hold-times     : Up 0 ms, Down 0 ms

  Current address: 48:5a:0d:b5:1c:57, Hardware address: 48:5a:0d:b5:1c:57

  Last flapped   : 2023-07-26 12:44:34 UTC (00:00:58 ago)

  Statistics last cleared: Never

  Traffic statistics:

   Input  bytes  :                 6992                  992 bps

   Output bytes  :                 6070                  992 bps

   Input  packets:                   73                    1 pps

   Output packets:                   61                    1 pps

   IPv6 transit statistics:

   Input  bytes  :                    0

   Output bytes  :                    0

   Input  packets:                    0

   Output packets:                    0

  Input errors:

    Errors: 0, Drops: 0, Framing errors: 0, Runts: 0, Policed discards: 0, L3 incompletes: 0, L2 channel errors: 0, L2 mismatch timeouts: 0, FIFO errors: 0, Resource errors: 0

  Output errors:

    Carrier transitions: 1, Errors: 0, Drops: 0, Collisions: 0, Aged packets: 0, FIFO errors: 0, HS link CRC errors: 0, MTU errors: 0, Resource errors: 0

  Egress queues: 10 supported, 5 in use

  Queue counters:       Queued packets  Transmitted packets      Dropped packets

    0                               61                   61                    0

    3                                0                    0                    0

    4                                0                    0                    0

    7                                0                    0                    0

    8                                0                    0                    0

  Queue number:         Mapped forwarding classes

    0                   best-effort

    3                   fcoe

    4                   no-loss

    7                   network-control

    8                   mcast

  Active alarms  : None

  Active defects : None

 Pre-emphasis(reg 236/237)

                       Register-value                 0

 Ctle(reg 234/235)

                    Register-value                 0

 Differential-amplitude(reg 238/239)

                        Register-value                 0

  PCS statistics                      Seconds

    Bit errors                             0

    Errored blocks                         0

  Ethernet FEC Mode  :                  FEC91

  Ethernet FEC statistics              Errors

    FEC Corrected Errors                    0

    FEC Uncorrected Errors                  0

    FEC Corrected Errors Rate               0

    FEC Uncorrected Errors Rate             0

  MAC statistics:                      Receive         Transmit

    Total octets                          6992             6070

    Total packets                           73               61

    Unicast packets                         60               59

    Broadcast packets                        4                2

    Multicast packets                        9                0

    CRC/Align errors                         0                0

    FIFO errors                              0                0

    MAC control frames                       0                0

    MAC pause frames                         0                0

    Oversized frames                         0

    Jabber frames                            0

    Fragment frames                          0

    VLAN tagged frames                       0

    Code violations                          0

  MAC Priority Flow Control Statistics:

    Priority :  0                             0                0

    Priority :  1                             0                0

    Priority :  2                             0                0

    Priority :  3                             0                0

    Priority :  4                             0                0

    Priority :  5                             0                0

    Priority :  6                             0                0

    Priority :  7                             0                0

  PRBS Mode : Disabled

  Packet Forwarding Engine configuration:

    Destination slot: 0 (0x00)

  CoS information:

    Direction : Output

    CoS transmit queue               Bandwidth               Buffer Priority   Limit

                              %            bps     %           usec

    0 best-effort             5     5000000000     5              0      low    none

    3 fcoe                   35    35000000000    35              0      low    none

    4 no-loss                35    35000000000    35              0      low    none

    7 network-control         5     5000000000     5              0      low    none

    8 mcast                  20    20000000000    20              0      low    none

  Interface transmit statistics: Disabled

  MACSec statistics:

    Output

        Secure Channel Transmitted

        Protected Packets               : 0

        Encrypted Packets               : 0

        Protected Bytes                 : 0

        Encrypted Bytes                 : 0

     Input

        Secure Channel Received

        Accepted Packets                : 0

        Validated Bytes                 : 0

        Decrypted Bytes                 : 0



  Logical interface et-0/0/0.0 (Index 554) (SNMP ifIndex 519) (HW Token 4095) (Generation 141)

    Flags: Up SNMP-Traps 0x4004000 Encapsulation: ENET2

    Traffic statistics:

     Input  bytes  :                 6982

     Output bytes  :                 5950

     Input  packets:                   72

     Output packets:                   63

    Local statistics:

     Input  bytes  :                 5872

     Output bytes  :                 5950

     Input  packets:                   72

     Output packets:                   63

    Transit statistics:

     Input  bytes  :                 1110                  808 bps

     Output bytes  :                    0                    0 bps

     Input  packets:                    0                    0 pps

     Output packets:                    0                    0 pps

    Protocol inet, MTU: 1500

    Max nh cache: 75000, New hold nh limit: 75000, Curr nh cnt: 1, Curr new hold cnt: 0, NH drop cnt: 0

    Generation: 161, Route table: 0

      Flags: Sendbcast-pkt-to-re, Is-Primary

      Addresses, Flags: Is-Default Is-Preferred Is-Primary

        Destination: 10.10.10/24, Local: 10.10.10.1, Broadcast: 10.10.10.255, Generation: 140



{master:0}

root@LAB_QFX5120-32C> ore 

  Link-level type: Ethernet, MTU: 1514, LAN-PHY mode, Speed: 100Gbps, BPDU Error: None, Loop Detect PDU Error: None, Ethernet-Switching Error: None, MAC-REWRITE Error: None, Loopback: Disabled, Source filtering: Disabled, Flow control: Disabled, Media type: Fiber

  Input errors:

    Errors: 0, Drops: 0, Framing errors: 0, Runts: 0, Policed discards: 0, L3 incompletes: 0, L2 channel errors: 0, L2 mismatch timeouts: 0, FIFO errors: 0, Resource errors: 0

  Output errors:

    Carrier transitions: 1, Errors: 0, Drops: 0, Collisions: 0, Aged packets: 0, FIFO errors: 0, HS link CRC errors: 0, MTU errors: 0, Resource errors: 0

    Bit errors                             0

    Errored blocks                         0

  Ethernet FEC statistics              Errors

    FEC Corrected Errors                    0

    FEC Uncorrected Errors                  0

    FEC Corrected Errors Rate               0

    FEC Uncorrected Errors Rate             0

    CRC/Align errors                         0                0

    FIFO errors                              0                0

      Addresses, Flags: Is-Default Is-Preferred Is-Primary



{master:0}

root@LAB_QFX5120-32C> ate 

  Input rate     : 1008 bps (1 pps)

  Output rate    : 1008 bps (1 pps)

    FEC Corrected Errors Rate               0

    FEC Uncorrected Errors Rate             0

  Input rate     : 0 bps (0 pps)

  Output rate    : 0 bps (0 pps)



{master:0}

root@LAB_QFX5120-32C> 100 

PING 10.10.10.2 (10.10.10.2): 56 data bytes

!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!

--- 10.10.10.2 ping statistics ---

100 packets transmitted, 100 packets received, 0% packet loss

round-trip min/avg/max/stddev = 0.882/7.647/8.427/1.377 ms



{master:0}

root@LAB_QFX5120-32C> ore 

Physical interface: et-0/0/0

    Module temperature                        :  34 degrees C / 94 degrees F

    Module voltage                            :  3.3350 V

    Module temperature high alarm             :  Off

    Module temperature low alarm              :  Off

    Module temperature high warning           :  Off

    Module temperature low warning            :  Off

    Module voltage high alarm                 :  Off

    Module voltage low alarm                  :  Off

    Module voltage high warning               :  Off

    Module voltage low warning                :  Off

    Module temperature high alarm threshold   :  80 degrees C / 176 degrees F

    Module temperature low alarm threshold    :  -10 degrees C / 14 degrees F

    Module temperature high warning threshold :  75 degrees C / 167 degrees F

    Module temperature low warning threshold  :  -5 degrees C / 23 degrees F

    Module voltage high alarm threshold       :  3.5990 V

    Module voltage low alarm threshold        :  2.9990 V

    Module voltage high warning threshold     :  3.4990 V

    Module voltage low warning threshold      :  3.0990 V

    Laser bias current high alarm threshold   :  14.999 mA

    Laser bias current low alarm threshold    :  0.999 mA

    Laser bias current high warning threshold :  12.999 mA

    Laser bias current low warning threshold  :  1.999 mA

    Laser output power high alarm threshold   :  3.5481 mW / 5.50 dBm

    Laser output power low alarm threshold    :  0.1259 mW / -9.00 dBm

    Laser output power high warning threshold :  3.1623 mW / 5.00 dBm

    Laser output power low warning threshold  :  0.1413 mW / -8.50 dBm

    Laser rx power high alarm threshold       :  1.7783 mW / 2.50 dBm

    Laser rx power low alarm threshold        :  0.0447 mW / -13.50 dBm

    Laser rx power high warning threshold     :  1.5849 mW / 2.00 dBm

    Laser rx power low warning threshold      :  0.0501 mW / -13.00 dBm

  Lane 0

    Laser bias current                        :  7.498 mA

    Laser output power                        :  1.196 mW / 0.78 dBm

    Laser receiver power                      :  1.059 mW / 0.25 dBm

    Laser bias current high alarm             :  Off

    Laser bias current low alarm              :  Off

    Laser bias current high warning           :  Off

    Laser bias current low warning            :  Off

    Laser receiver power high alarm           :  Off

    Laser receiver power low alarm            :  Off

    Laser receiver power high warning         :  Off

    Laser receiver power low warning          :  Off

    Tx loss of signal functionality alarm     :  Off

    Rx loss of signal alarm                   :  Off

    Tx laser disabled alarm                   :  Off

  Lane 1

    Laser bias current                        :  7.978 mA

    Laser output power                        :  1.312 mW / 1.18 dBm

    Laser receiver power                      :  1.125 mW / 0.51 dBm

    Laser bias current high alarm             :  Off

    Laser bias current low alarm              :  Off

    Laser bias current high warning           :  Off

    Laser bias current low warning            :  Off

    Laser receiver power high alarm           :  Off

    Laser receiver power low alarm            :  Off

    Laser receiver power high warning         :  Off

    Laser receiver power low warning          :  Off

    Tx loss of signal functionality alarm     :  Off

    Rx loss of signal alarm                   :  Off

    Tx laser disabled alarm                   :  Off

  Lane 2

    Laser bias current                        :  8.180 mA

    Laser output power                        :  1.403 mW / 1.47 dBm

    Laser receiver power                      :  0.958 mW / -0.19 dBm

    Laser bias current high alarm             :  Off

    Laser bias current low alarm              :  Off

    Laser bias current high warning           :  Off

    Laser bias current low warning            :  Off

    Laser receiver power high alarm           :  Off

    Laser receiver power low alarm            :  Off

    Laser receiver power high warning         :  Off

    Laser receiver power low warning          :  Off

    Tx loss of signal functionality alarm     :  Off

    Rx loss of signal alarm                   :  Off

    Tx laser disabled alarm                   :  Off

  Lane 3

    Laser bias current                        :  7.737 mA

    Laser output power                        :  1.219 mW / 0.86 dBm

    Laser receiver power                      :  1.075 mW / 0.32 dBm

    Laser bias current high alarm             :  Off

    Laser bias current low alarm              :  Off

    Laser bias current high warning           :  Off

    Laser bias current low warning            :  Off

    Laser receiver power high alarm           :  Off

    Laser receiver power low alarm            :  Off

    Laser receiver power high warning         :  Off

    Laser receiver power low warning          :  Off

    Tx loss of signal functionality alarm     :  Off

    Rx loss of signal alarm                   :  Off

    Tx laser disabled alarm                   :  Off



{master:0}

root@LAB_QFX5120-32C> re 

Physical interface: et-0/0/0

    Module temperature                        :  35 degrees C / 94 degrees F

    Module voltage                            :  3.3330 V

    Module temperature high alarm threshold   :  80 degrees C / 176 degrees F

    Module temperature low alarm threshold    :  -10 degrees C / 14 degrees F

    Module temperature high warning threshold :  75 degrees C / 167 degrees F

    Module temperature low warning threshold  :  -5 degrees C / 23 degrees F

    Module voltage high alarm threshold       :  3.5990 V

    Module voltage low alarm threshold        :  2.9990 V

    Module voltage high warning threshold     :  3.4990 V

    Module voltage low warning threshold      :  3.0990 V

    Laser bias current high alarm threshold   :  14.999 mA

    Laser bias current low alarm threshold    :  0.999 mA

    Laser bias current high warning threshold :  12.999 mA

    Laser bias current low warning threshold  :  1.999 mA

    Laser output power high alarm threshold   :  3.5481 mW / 5.50 dBm

    Laser output power low alarm threshold    :  0.1259 mW / -9.00 dBm

    Laser output power high warning threshold :  3.1623 mW / 5.00 dBm

    Laser output power low warning threshold  :  0.1413 mW / -8.50 dBm

    Laser rx power high alarm threshold       :  1.7783 mW / 2.50 dBm

    Laser rx power low alarm threshold        :  0.0447 mW / -13.50 dBm

    Laser rx power high warning threshold     :  1.5849 mW / 2.00 dBm

    Laser rx power low warning threshold      :  0.0501 mW / -13.00 dBm

  Lane 0

    Laser bias current                        :  7.817 mA

    Laser output power                        :  1.242 mW / 0.94 dBm

    Laser receiver power                      :  1.060 mW / 0.25 dBm

  Lane 1

    Laser bias current                        :  8.020 mA

    Laser output power                        :  1.318 mW / 1.20 dBm

    Laser receiver power                      :  1.128 mW / 0.52 dBm

  Lane 2

    Laser bias current                        :  8.140 mA

    Laser output power                        :  1.397 mW / 1.45 dBm

    Laser receiver power                      :  0.958 mW / -0.18 dBm

  Lane 3

    Laser bias current                        :  7.777 mA

    Laser output power                        :  1.225 mW / 0.88 dBm

    Laser receiver power                      :  1.077 mW / 0.32 dBm



{master:0}

root@LAB_QFX5120-32C